[video member=miotatsu stream_platform=twitch project=riscy title="Programming the HiFive1" vod_platform=youtube id=Y0m1sW2oQVY annotator=Miblo]
[0:06][Recap and set the stage for the day]
[1:32][Begin to acquaint ourselves with the demo code from the Freedom E SDK]
[2:47][Take a look at plic_driver.h and .c]
[13:26][Return to demo_gpio.c]
[25:28][@miblo][Are there two stages to the interrupt: claim_interrupt() and actual_interrupt() or whatever?]
[25:46][@miblo][So both of them do 1.5 seconds which add up to 3?]
[27:24][Determine to try uploading this demo program to the HiFive1]
[28:02][I am grounded once again][quote 9]
[29:24][Connect to the HiFive1 and try uploading demo_gpio]
[32:20][Compile demo_gpio and try uploading that]
[33:56][@miblo][@miotatsu: PROGAM is misspelled]
[34:50][Reconnect to the HiFive1 and try out the demo]
[37:09][@miblo][I mean, surely that missing R can't have made it partially succeed...]
[37:30][Try killing screen and reconnecting to it]
[38:15][Tweak hello.c, compile and hit an error]
[42:35][Try modifying demo_gpio.c instead]
[50:16][@miblo][You could just do: $^v}A\\n\\]
[50:47][@quartertron][You could just do \@a then hold down \@ until you get where you wanna be]
[51:39][Rebuild demo_gpio and upload it]
[52:16][Congratulate @Miblo for being the first person to be slammed a thunderous high-five by the HiFive1]
[52:58][This is all we have time for today]
[/video]
