[video member=miotatsu stream_platform=twitch project=riscy medium=drawing title="RISC-V PC Model & Starting on Case" vod_platform=youtube id=CI-8Hem7qLs annotator=Miblo]
[0:01][Recap our code cleanup since last time]
[1:36][:Research the Craftcloud 3D printing service[ref
    site=Craftcloud
    url=https://www.craftcloud3d.com/]]
[11:09][:Research the JawsTec 3D printing service[ref
    site=JawsTec
    url=https://jawstec.com/]]
[14:14][:Research the Autotiv 3D printing service[ref
    site=Autotiv
    url=https://autotiv.com/]]
[17:07][Thoughts on the expense of our case][:speech]
[18:48][Plug our updates to links.riscy.tv[ref
    site=links.riscy.tv
    url=http://links.riscy.tv/]][:research]
[26:10][Determine to finish the RISC-V PC model before starting on the case][:speech]
[27:21][Measure the notch on the Graphics card (8mm)][:admin]
[30:21][Fix the vertical position of the Graphics card's bracket to account for the notch]
[33:03][Roughly position the Graphics card in our full model]
[34:14][Determine to model the Expansion Board's PCI-e ×16 connector, initially cutting out a region to accommodate it]
[41:38][Measure the Expansion Board's PCI-e ×16 connector (89mm)][:admin]
[46:32][Model the Expansion Board's PCI-e ×16 connector]
[52:25][Measure the x position of the Expansion Board's PCI-e ×16 connector (12.5mm)][:admin]
[54:27][Position the Expansion Board's PCI-e ×16 connector in x]
[54:59][Measure the y position of the Expansion Board's PCI-e ×16 connector (28mm)][:admin]
[56:44][Position the Expansion Board's PCI-e ×16 connector in y]
[59:13][Measure from the other edge the y position of the Expansion Board's PCI-e ×16 connector (3.5mm)][:admin]
[1:02:52][Fix the y position of the Expansion Board's PCI-e ×16 connector]
[1:04:55][Slot the Graphics card and Expansion Board together, fixing the connector location]
[1:15:54][Plug our real life Graphics card into the Expansion Board to confirm that it lines up with the USB card][:admin]
[1:19:14][Lower the Graphics card into place]
[1:22:31][Express concern about our Expansion Board dimensions]
[1:24:40][Double-check the Expansion Board y dimension (120mm)][:admin]
[1:27:22][Fix our Expansion Board's y dimension from 117mm to 120mm]
[1:29:13][Double-check the Expansion Board's x dimension (272mm)][:admin]
[1:30:28][Consider our RISC-V PC model to be provisionally done]
[1:32:55][Double-check and fix the position of our Expansion Board's PCI-e ×16 connector][:admin :drawing]
[1:39:10][Break][:admin]
[1:39:21][Return and fix the position of our Graphics card]
[1:42:14][Double-check and fix the position of our Expansion Board's PCI-e ×1 connector][:admin :drawing]
[1:55:40][Double-check the x dimension of our USB card's PCI-e ×1 connector (20mm)][:admin]
[1:58:54][Slide the USB card into position, within its wiggle room]
[2:01:55][Double-check the position of our Expansion Board's FMC connector and HiFive Unleashed][:admin]
[2:08:43][Double-check the positions of our Expansion Board's stand-offs][:admin]
[2:15:44][Introduce guts() module to house our whole model]
[2:16:18][Embark on modelling the case[ref
    site=Autotiv
    page="Selective Laser Sintering (SLS)"
    url=https://autotiv.com/selective-laser-sintering]]
[2:34:09][Model the case's stand-offs]
[2:41:50][Raise the end area of the case to meet the HiFive Unleashed]
[2:59:19][:Research OpenSCAD's offerings in terms of our sloped surface[ref
    site=OpenSCAD
    page="Cheat sheet"
    url=https://www.openscad.org/cheatsheet/index.html][ref
        site=WikiBooks
        page="OpenSCAD User Manual/Transformations#hull"
        url=https://en.wikibooks.org/wiki/OpenSCAD_User_Manual/Transformations#hull][ref
            site=WikiBooks
            page="OpenSCAD User Manual/Using_the_2D_Subsystem#Rotate_Extrude"
            url=https://en.wikibooks.org/wiki/OpenSCAD_User_Manual/Using_the_2D_Subsystem#Rotate_Extrude][ref
            site=WikiBooks
            page="OpenSCAD User Manual/Primitive_Solids#Cylinder"
            url=https://en.wikibooks.org/wiki/OpenSCAD_User_Manual/Primitive_Solids#Cylinder]]
[3:07:36][Produce our case's sloped surface out of a cylinder()]
[3:26:00][Determine to model the raised surface, also consider making the case's stand-offs smaller]
[3:27:17][Don the antistatic wristband, and measure our stand-off screw (2.3mm)][:admin]
[3:29:26][Reduce our case's stand-off screws from 3.5mm to 3mm diameter]
[3:30:04][Model the case's raised surface]
[3:35:31][Consider namespacing our code[ref
    site=WikiBooks
    page="OpenSCAD User Manual/General#Variables"
    url=https://en.wikibooks.org/wiki/OpenSCAD_User_Manual/General#Variables]][:research]
[3:38:59][Scope our stand-off code]
[3:40:32][Call it a day][:speech]
[/video]
